---------------------
Version Information
---------------------
SonixUVCDriver (NoLogo)  
    Driver  6.0.1324.22

----------------------------
Silent Installation Command 
----------------------------
Run "<path\>setup.exe -s"
i.e. c:\myfolder\setup.exe -s

-------------------------------
Silent Uninstallation Command
-------------------------------
Run "<path\>setup.exe -removeonly -s"
i.e. c:\myfolder\setup.exe -removeonly -s

--------------------
Support Languages
--------------------
Basque, Bulgarian, Catalan
Chinese-Simplified, Chinese-Traditional-TW
Croatian, Czech, Danish, Dutch
English, Finnish, French
French/Canadian, German, Greek
Hungarian, Indonesian, Italian
Japanese, Korean, Norwegian
Polish, Portuguese/Brazil
Portuguese/Portugal, Romanian
Russian, Serbian, Slovak, Slovenian
Spanish, Swedish, Thai, Turkish

--------------------
Changed History
--------------------
v6.0.1312.10
1)First release
2)Add new VID/PID: 0x0C45/0x6513

v6.0.1313.0
1)2nd release
2)Fix: a. MJPEG @ <VGA resolution black screen
       b. YUV @ <VGA resolution FaceAE no action
       c. @ 800x600 resolution, frame of FaceAE crooked

v6.0.1313.1
1)3rd release
2)Add new VID/PID: 0x0C45/0x6514

v6.0.1314.0
1)4th release
2)Add AutoFlicker
3)Add Privacy Shield
4)Remove C:\\setup.log after install
5)Chang to One-Button-Install
6)Known issue: a. Randomly show crash bugcheck50 when closing stream
               b. WHCK CHOAS Fail (Both CAMERA and COMPOSITE Fail)

v6.0.1316.0
1)Fix issue: a. Randomly show crash bugcheck50 when closing stream
             b. WHCK CHOAS Fail (Both CAMERA and COMPOSITE Fail)
	     c. WHCK BasicPerf fail

v6.0.1316.1
1)Fix checkinf fail in #341

v6.0.1317.0
1)Set auto antiflicker default value as 0:auto
2)Remove setup.iss

v6.0.1317.4
1)WHQLed driver version
2)Complete dialog after driver installation and restart
3)Silent uninstall during driver uninstallation from control panel

v6.0.1317.6
1)Multi-Language support in property page
2)Fix a protential crash while streaming small image(<VGA)

v6.0.1317.8
1)Fix Win7 property page incorrect value of FaceAE and low light
2)Fix BSOD while doing Device WHQL PnP 

v6.0.1317.9
1)Fix randomly BSOD 0x50 while streaming small resolution.

v6.0.1318.1 (debug version)
1)Fix 160x120 drop frame issue
2)Set auto anti-flicker start from 50hz
3)Fix auto anti-flicker not working issue, change params of auto anti-flicker.

v6.0.1318.2
1)Fix BSOC 0x50 while doing system pnp and sleep with IO test

v6.0.1318.3
1)Fix QQ crash while streaming MJPG vga

v6.0.1318.9
1)Fix QQ crash while streaming MJPG vga(renew version of 6.0.1318.3)
2)Fix Auto AntiFlicker function fail.

v6.0.1319.1
1)Fix system WHCK test sleep and pnp BSOD issue

v6.0.1319.9
1)調整AAF參數提高準確度
2)系統system performance測項的修正

v6.0.1320.1
1)AAF check OK
2)Bypass system performance frame 20 seconds

v6.0.1320.2
1) Fixed that Metro camera AP has garbage preview image when recording video.

v6.0.1320.3
1)Fix HCK 測試項 Driver memory fail
2)Fix HCK 測試項 System performace fail

v6.0.1320.4
1)修正Control Panel Uninstall畫面閃動問題

v6.0.1320.6
1)移除Control Panel Uninstall對話框

v6.0.1320.8
1)修正客戶影像異常問題

v6.0.1320.9
1)Cancel FaceAE option on Win7

v6.0.1321.0
1)Win8 0.1M resolution preview sometimes green scene

v6.0.1323.0
1)Fix BSOD issue
2)Fix cpu rate too high when previewing YUV issue

v6.0.1323.1
1)when privacy function on, show LENOVO graph

v6.0.1323.2
1)修改property page顯示文字內容

v6.0.1324.7
1)修正Cancel鍵對FaceAE無作用
2)修正某些情形下，重開機後，Video Qality錯誤問題

v6.0.1324.21_DEBUG
客戶回覆重複disable/enable數次device，系統BSOD
但因SONIX端無法複製，故提供DEBUG版本供客戶測試
若客戶端利用此版本測試發生BSOD時，能提供SONIX端kernel message及Dump File
1) 利用客戶提供Dump file，看到一問題: 帶入privacy function的其中一項參數，length = 0 (正確應不為0)
2) 針對(1)敘述作猜測性修改

v6.0.1324.22
1) 修正客戶回覆重複disable/enable，系統BSOD問題
2) root cause: 因buffer大小為640*480*2，但因preview HD，access buffer時，access到超過buffer大小記憶體